Oct 7, 2016 Tom O’Riley wrote:

                     ISI ID      serial#            sync time

300 KHz Workhorse    1825       WHS300-1-UG521      10/07/2016 20:48:00 UTC
600 KHz Workhorse    1828       WHS1200-I-UG515     10/07/2016 20:53:00 UTC
Aquadopp             1474       AQD1995             10/07/2016 21:45:50 UTC

Notes: 
The Seabird CTD has an internal clock, but is not used for 'streaming mode'.
The 1200 KHz Workhorse is still at sea on BIN #2, we'll sync its clock after its recovered
The WETLabs Triplet has an internal clock but doesn't log data internally. Ignore WETLabs clock, use SIAM timestamp instead.

Oct 17, 2016 Tom O’Riley wrote:
And today we synced the 1200KHz Workhorse clock:

                     ISI ID      serial#            sync time

1200 KHz Workhorse   1827        20662              10/17/2016 17:28 UTC